Products

## Euro Mortise Lock

Impotent Features & Benefits
•Conforms to the requirements of EN12209-3
•Single or triple deadbolts with one or two throws.
•Quick reversible latch for easy on-site handing.
•Reversible latch bolts can be optioned to be operating by key or handle.
•3point latch to enable smooth and quite closing . Also can prevent door from slamming.
•Adjustable roller latch. Hook latch for steel door or pull gate.
•Large range of cylinders conforming to EN1303 with various features. •The KA and MK/GMK are available
Face plate:
•Material: Stainless steel 201 304 316
•Type: round head / square head
•Thickness: 3mm,Width: 22mm
•Finish: SS/SP/AB/AC/ PVD
Striker plate:
•Material: Stainless steel 201 304 316
•1.2mm thickness, 1.5mm available
•Finish: SS/SP/AB/AC/ PVD
Lock case:
•Material: Steel, 1.2mm thickness
•Electrolysis board/Yellow crackle/Silver board/Black crackle/ Snow-flake board.

Euro Mortise lock with dead bolt
Item No. | Centre distance | E | A | Follower | Throws
ML85.40.B | 85 | 40 | 67 | 8 | 2
ML85.45.B | 85 | 45 | 72 | 8 | 2
ML85.50.B | 85 | 50 | 77 | 8 | 2
ML85.60.B | 85 | 60 | 87 | 8 | 2

Euro Mortise lock with latch bolt
Item No. | Centre distance | E | A | Follower | Throws
ML85.40.L | 85 | 40 | 67 | 8 | -
ML85.45.L | 85 | 45 | 72 | 8 | -
ML85.50.L | 85 | 50 | 77 | 8 | -
ML85.60.L | 85 | 60 | 87 | 8 | -

Euro Mortise lock with dead bolt and latch bolt
Item No. | Centre distance | E | A | Follower | Throws
ML85.40.LB | 85 | 40 | 67 | 8 | 2
ML85.45.LB | 85 | 45 | 72 | 8 | 2
ML85.50.LB | 85 | 50 | 77 | 8 | 2
ML85.60.LB | 85 | 60 | 87 | 8 | 2

Euro Mortise lock with dead bolt and 3point latch bolt
•3point latch to enable smooth and quite closing. Also can prevent door from slamming.
Item No. | Centre distance | E | A | Follower | Throws
ML85.40.3LB | 85 | 40 | 67 | 8 | 2
ML85.45.3LB | 85 | 45 | 72 | 8 | 2
ML85.50.3LB | 85 | 50 | 77 | 8 | 2
ML85.60.3LB | 85 | 60 | 87 | 8 | 2

Euro Mortise lock with latch bolt and dead bolt by emergency release
•T he latch and deadbolt operated by handle inside quickly at the same time as the emergency release
Item No. | Centre distance | E | A | Follower | Throws
ML85.60.LBE | 85 | 60 | 89 | 8 | 2

Euro Mortise lock with latch bolt by emergency release
•LE-1 The latch operated by key outside or handle inside
•LE-2 The latch operated by key outside or handle both side
•Latch, Face plate, Strike plate are stainless steel
•LE-1 Especially suitable for storeroom
•LE-2 Especially suitable for classroom/meeting room/office room
Item No. | Centre distance | E | A | Follower | Throws
ML85.60.LE-1 | 85 | 60 | 89 | 8 | -
ML85.60.LE-2 | 85 | 60 | 89 | 8 | -

Euro Mortise lock with triple square deadbolts and latch bolt
Item No. | Centre distance | E | A | Follower | Throws
ML85.45.L3B | 85 | 45 | 72 | 8 | 2
ML85.50.L3B | 85 | 50 | 77 | 8 | 2
ML85.60.L3B | 85 | 60 | 87 | 8 | 2

Euro Mortise lock with triple round deadbolts and latch bolt
•Latch, deadbolt, Face plate, Strike plate are stainless steel
Item No. | Centre distance | E | A | Follower | Throws
ML85.50.L3RB | 85 | 50 | 77 | 8 | 2
ML85.60.L3RB | 85 | 60 | 87 | 8 | 2

Euro Mortise lock with triple round deadbolts and roller latch
•L atch, Face plate, Strike plate are stainless steel
Item No. | Centre distance | E | A | Follower | Throws
ML85.50.L3RB | 85 | 50 | 77 | 8 | 2
ML85.60.L3RB | 85 | 60 | 87 | 8 | 2

Euro Mortise lock with deadbolts and roller latch
Item No. | Centre distance | E | A | Follower | Throws
ML85.40.RLB | 85 | 40 | 67 | 8 | 2
ML85.45.RLB | 85 | 45 | 72 | 8 | 2
ML85.50.RLB | 85 | 50 | 77 | 8 | 2
ML85.60.RLB | 85 | 60 | 87 | 8 | 2
ML85.70.RLB | 85 | 70 | 97 | 8 | 2

Euro Mortise lock narrow body with dead bolt and latch bolt
Item No. | Centre distance | E | A | Follower | Throws
ML85.20.LB | 85 | 20 | 37 | 8 | 1
ML85.25.LB | 85 | 25 | 42 | 8 | 1
ML85.30.LB | 85 | 30 | 47 | 8 | 1
ML85.35.LB | 85 | 35 | 52 | 8 | 1

Euro lock with hook latch
•After the latch locked by key, the handle can not operated anymore
•Suitable for pull gate or steel door
•Latch, Face plate, Strike plate are stainless steel
Item No. | Centre distance | E | A | Follower | Throws
ML70.30.HL | 70 | 30 | 60 | 8 | -
ML70.40.HL | 70 | 40 | 70 | 8 | -
ML70.50.HL | 70 | 50 | 80 | 8 | -
ML70.60.HL | 70 | 60 | 90 | 8 | -

Euro lock heavy duty with hook latch and orientated pins
•After the latch locked by key, the handle can not operated anymore
•Suitable for pull gate or steel door
•Latch, Face plate, Strike plate are stainless steel
Item No. | Centre distance | E | A | Follower | Throws
ML72.50.HLB | 72 | 50 | 86 | 8 | -
ML72.60.HLB | 72 | 60 | 96 | 8 | -
ML72.70.HLB | 72 | 70 | 106 | 8 | -