Products

## Rolling Shutter Lock

Cylinder Lock For Rolling Shutter

1. Single turn, 3 pins cylinder lock
2. Interchangeable: With most common roller shutter locks available on the market. The reinforced bolt makes the roller shutter more
3. resistant to attack.
4. Available for motorized roller shutter
5. Reinforced steel bolt: 2mm steel plated folded back on itself to reach overall 6.5mm thickness
6. Straight, shifted, Lengthened bolt available with 6mm hole
7. Solid brass cylinder
8. Rustproof zinc plated box and components
9. *3 brass key, chromed plated

CL01.01: Double straight bolt
Item No. A B PINS FINISH QTY/BOX
CL01.01 155 56 3 GALVANIZED 6

CL01.02: Double shifted bolt
Item No. A B PINS FINISH QTY/BOX
CL01.02 155 56 3 GALVANIZED 6
CL01.03: Right side straight bolt
Item No. A B PINS FINISH QTY/BOX
CL01.03 155 56 3 GALVANIZED 6

CL01.04: Right side shifted bolt
Item No. A B PINS FINISH QTY/BOX
CL01.04 155 56 3 GALVANIZED 6

CL01.05: Left side straight bolt
Item No. A B PINS FINISH QTY/BOX
CL01.05 155 55 3 GALVANIZED 6

CL01.06: Left side shifted bolt
Item No. A B PINS FINISH QTY/BOX
CL01.06 155 55 3 GALVANIZED 6

Cylinder Lock Set For Rolling Shutter
1. 1 right + 1 left = 1 pair
2. 1 pair = KEY ALIKE
3. Supply 3 keys for 1 pair
4. Single turn, 3 pins cylinder lock
5. Interchangeable: With most common roller shutter locks available on the market. The reinforced bolt makes the roller shutter more resistant to attack.
6. Available for motorized roller shutter
7. Reinforced steel bolt: 2mm steel plated folded back on itself to reach overall 6.5mm thickness
8. Straight, shifted, Lengthened bolt available with 6mm hole
9. Solid brass cylinder
10.Rustproof zinc plated box and components
11.*3 brass key, chromed plated

CL01.07: Straight bolt (CL503+CL505)

Item No. | A | B | PINS | FINISH | QTY/BOX
CL01.07 | 155 | 55 | 3 | GALVANIZED | 6

CL01.08: Shifted bolt (CL504+CL506)

Item No. | A | B | PINS | FINISH | QTY/BOX
CL01.08 | 155 | 55 | 3 | GALVANIZED | 6