Products

## Cylinder Locks For Up&Over Garage Doors

1. Handle square 8mm 2. Unlocking lever 3. Bolt with 6mm hole is optional 4. Single turn, 4 pins cylinder lock 5. Interchangeable: With most common roller shutter locks available on the market. The reinforced bolt makes the roller shutter more resistant to attack 6. Reinforced steel bolt: 2mm steel plated folded back on itself to reach overall 6.5mm thickness 7. Stright, shifted, Lengthened bolt available with 6mm hole 8. Solid brass cylinder 9. Rustproof zinc plated box and components 10.3 brass key, chromed plated
CL01.09: with fixed round cylinder
Item No. | A | B | PINS | FINISH | QTY/BOX
CL01.09 | 155 | 56 | 4 | GALVANIZED | 6
| CL01.10： Lock body for Euro cylinder
Item No. | A | B | PINS | FINISH | QTY/BOX
CL01.10 | 155 | 56 | 4 | GALVANIZED | 6