Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# 95% Nano Zinc Oxide (20-100nm)

- Previous
- Next

95% Nano Zinc Oxide (20-100nm)

It's a kind of fine white or yellowish powder, with average particle size of about 30 nanometers, size range of 10 ~ 40 nm, compared with zinc oxide with direct and indirect method, it has a tiny grains, big specific surface area, and is easy to disperse, Our nanometer zinc oxide is refined from the ammonia - ammonium gel precipitation, mainly used to replace the zinc oxide by direct and indirect method, and used for a variety of natural rubber and synthetic rubber vulcanizing agent and reinforcing agent, white colored glue stains and filling agent, it can reduce the dosage of 30 ~ 50%,can also be widely used in all kinds of foam products, paint additives, feed additives, ceramic glaze, galvanized material, metal surface treatment phosphating liquid additives, cosmetics, catalysts, enamel, medicine, electronic sensors, antistatic material, etc.

GB/T9589-2004 Standard

I tem | Index
First Class | Second | Third
ZnO% ≥ | 99.0 | 97.0 | 95.0
Average Dia/nm ≤ | 100 | 100 | 100
XRD average grain size/nm ≤ | 100 | 100 | 100
Area size(m3/g) ≥ | 15 | 15 | 35
Aggregate stability index≤ | 100 | 100 | 100
(Pb)/% ≤ | 0.001 | 0.001 | 0.03
(Mn)/% ≤ | 0.001 | 0.001 | 0.005
(Cu)/% ≤ | 0.0005 | 0.0005 | 0.003
(Cd)% ≤ | 0.0015 | 0.005 | -
(Hg)/% ≤ | 0.0001 | - | -
(As)/% ≤ | 0.0003 | - | -
105℃ Volatile matter /% ≤ | 0.5 | 0.5 | 0.7
Water soluble matter /% ≤ | 0.10 | 0.10 | 0.7
HCL insoluble matter/% ≤ | 0.02 | 0.02 | 0.05
Loss on ignition/% ≤ | - | 2 | 4

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.