Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# Sodium Silicate for textile printing

- Previous

Product name: Sodium Silicate

CAS No.: 1344-09-8
EINECS No.:215-687-4
Molecular Weight:100.0814
Molecular Formula:Na2SiO3

ITEM | Liquid
20 | 2.8 | 3.2 | 3.6 | 4.0 | 3.4
Density(g/cm3,20℃) | 1.543~1.599 | 1.422~1.436 | 1.381~1.394 | 1.318~1.33 | 1.245~1.257 | 1.296~1.308
Degree Baum′e(°Be,20℃) | 50.0~51.0 | 43.0~44.0 | 40.0~41.0 | 35.0~36 | 28.5~29.5 | 33.0~34.0
K2O ≥ % | 19.50 | 13.00 | 11.50 | 9.00 | 7.00 | 9.00
Sio2 ≥ % | 26.00 | 24.00 | 25.00 | 22.00 | 19.00 | 20.00
Modulus(M) | 2.00~2.20 | 2.80~3.00 | 3.15~3.35 | 3.5~3.7 | 3.90~4.10 | 3.30~3.50
Soluble silicate≥ % | - | - | - | - | - | -
S ≤ % | 0.030 | 0.030 | 0.030 | 0.030 | 0.030 | 0.030
Viscosity（Pa·S,20℃） | - | - | 0.80 | 0.15 | - | -

Application:
It's mainly used in refractory spraying material, refractory castables and other refractory materials.

Adhesion agent for thermal insulation material and acid proof mortar; thickener for oil field drilling industry;

and can also be used in coating industry, washing industry, soap industry and synthetic detergent as degreaser,

filler and buffer, etc.
Storage & Transportation
1. Storage and transportation
2. Keep in dry, cool and well-ventilated warehouse.
3. To protect from rain and damp; handle with care.
4. Use of once unpack or vacuum seal, to protect from damp.
Package: 25kg /pp/pe net bag(21MT/FCL).

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.