Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- 碱式碳酸锌
  - 油田专用
  - 橡胶专用
- 氧化锌
  - 间接法氧化锌
  - 直接法氧化锌
  - Particle Zinc Oxide
  - Nano Active Zinc Oxide
  - Feed Grade Zinc Oxide

###
Products

# Particle Zinc Oxide

- Previous
- Next

Description

Particle Zinc Oxide

Molecular formula: Zno
Molecular weight: 81.834
Performance: The products of modality made by Shun Pu is carrier-free micro granulation, no dust pollute, diameter of uniform size, physical mobility is good, hardness is good, benefit for long distance transport and modern measure, easy to melt, and easily mix with other materials.
Characteristic: 1. Reduce sulfur process and sulfur rubber use of zinc damage to the environment.
2. Carrier-free micro granulation effectively reduce dust pollution.
3.particles diameter is small, light transmittance is good, using in color and translucent rubber products can save materials.
4.particles diameter is small, but larger than superficial area, more easily dispersed on the rubber. by using unique technological, do not use the abrasive and squeezed, so can keep good dispersity. By using activated zinc oxide can increasing expand strength, tear strength and heat conductivity.
5.Enviromental making, using less energy resource in making procedure, reduce to waste energy, the duty of care for ecological.
Usage: Used mainly in rubber, ceramics, glass, cables and high added industries
Packaging: Polypropylene plastic woven bags or paper bags, in plastic bag of film, Each bag net weight 25kg.
Qualification:

Item | Qualification
type | SP-N1 | SP—N2
（ZnO）/% ≥ | 90 | 75
average grain diameter / cm | 0.1 | .01
Superficial area/（m²/g） ≥ | 50 | 50
agglomeration index num. ≤ | 100 | 100
Pb/% ≤ | 0.01 | 0.03
Mn/ % ≤ | 0.001 | 0.005
Cu/% ≤ | 0.001 | 0.003
Cd% ≤ | - | -
Hg/% ≤ | - | -
As/% ≤ | - | -
105°Cvolatile/% | 0.6 | 0.7
hydrotrope/% ≤ | 0.5 | 0.7

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.