Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# 76% Feed Grade Zinc Oxide

- Previous

76% Feed Grade Zinc Oxide

Physical and chemical properties:
Molecular formula: ZnO
Molecular Weight: 81.38
Appearance: Yellow powder
Bulk Density: About 0.6-0.8g/ml
Odor: .Odorless.
Solubility: Insoluble in water, alcohol; soluble in dilute acids.
Specific Gravity: 5.67
PH: No information found.
Melting Point: 1975℃ (3587F)
● High content of Zinc is favorable to reduce animal diarrhea and ablactation, as well as to improve propagation.
● Zinc Oxide has the function of sterilization and constringency. It has high surface activity and energy level due to fine particles and large specific surface area.

Items | Spec
Zn | ≥76.3%
ZnO | ≥95%
Pb | ≤10ppm
Cd | ≤8ppm
As | ≤5ppm
Screen residues through 150μm mesh | ≥99%

I ndex: The harmful elements such as Pb, Cd, As can achieve EU standard

Storage and Stability

Sensitive to, heat, light and moisture.

The product should be contained in unopened original package, protected from light in a dry place at low temperature ( no more than 15°C ). Once it is opened, please use it up in a short time.

The shelf life is 24 months for the unopened product stored in recommended condition.

Packaging

Inside: vacauumed aseptic PE bags, 20kg per bag.

Outside: kraft paper bag or carton

Packages size can also be offered according to customer requirement.

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.