欢迎光临石家庄市百胜化工有限责任公司！

> ### 产品目录

- 碱式碳酸锌
  - 油田专用
  - 橡胶专用
- 氧化锌
  - 间接法氧化锌
  - 直接法氧化锌
  - 纳米活性氧化锌
  - 饲料级别氧化锌
- 碳酸钾
  - 工业级
- 硬脂酸
  - 工业级
  - 工业级
  - 工业级
- 钛白粉
  - 金红石钛白粉
  - 锐钛型钛白粉
- 纯碱
  - 轻质纯碱
  - 重质纯碱

###
产品展示

# 金红石钛白粉

- 下一条

Molecular Formula: TiO2

Molecular Weight: 79.83

CAS No.: 13463-67-7

Apperance: White Power

Packaging Detail: PP bag with double layers of polyethlene film bag inside, 25kg per bag.

Delivery Detail: Within 15-20 days after receiving the payment.
Property: Titanium Dioxide has very low impurities, TIO2 particle size distribution is narrow,The membrane layer is continuous, uniform and dense, with high weatherability, high dispersion, high brightness and excellent scattering force.

Quality Standard: Q/3201 NTH 03-2011 (ISO591-1:2000:A1)

Application: Widely used in Plastic and rubber, paint, coatings, printing ink, glass, leather, cosmetics, soaps, and paper making etc.

Items | Spec
TiO2 content | ≥94%
Rutile type conversion rate | ≥97%
Whiteness | ≥95%
Tint Redusing Power，compared with standard sample | ≥100%
105℃ Volatile matter | ≤0.8%
Oil Absorption(g/100g) | ≤23
45 um sieve residue | ≤0.05%
PH value of aqueous suspension | 6.5-8.0
Hiding power | ≤25
Water-soluble Matter | ≤0.5%

Copyright © 石家庄市百胜化工有限责任公司 版权所有