Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# Potassium Carbonate

Molecular Formula: K2CO3

Molecular Weight: 138.21

CAS No.: 584-08-7

Appearance: Potassium Carbonate may be monoclinic crystal, white powder, granular crystal or prill.

Packaging Detail: PP bag with double layers of polyethlene film bag inside, 25kg per bag.

Delivery Detail: Within 15-20 days after receiving the payment.

Qality Standard: GB9103-88

Application:

i. ceramics

ii. glass

iii. explosives

iv.fertilizers,and glazes industry

v. in the the manufacture of soft soaps

vi. inorganic salts, and in dyeing and wool finishing.

Characteristics | Type I | Type II
High-class products | First-class products | Qualified products
Potassium carbonate content (K2CO3) | % ≥ | 99.0 | 98.5 | 96.0 | 99.0
Chloride content (KCl) | % ≤ | 0.01 | 0.10 | 0.20 | 0.03
Sulfur compound content (K2SO4) | % ≤ | 0.01 | 0.10 | 0.15 | 0.04
Ferrum content (Fe) | % ≤ | 0.001 | 0.003 | 0.010 | 0.001
Water insoluble content | % ≤ | 0.02 | 0.05 | 0.10 | 0.04
Loss from coal fire | % ≤ | 0.60 | 1.00 | 1.00 | 0.80
Notes: ignition loss index is for inspection during product packaging.

Handling and Storage: avoid sunlight, rain or moisture during transport.

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.