Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# Thermal protection catalyst

- Previous
- Next

This product is a high temperature thermal protective agent with alumina as the carrier and nickel as the active component.

The product and the conversion catalyst are used for the top of the gaseous hydrocarbon two-stage conversion furnace as heat protectant.

This product ADAPTS to the specific operating environment and conditions of the top of the reformer furnace, and can withstand high temperature and airflow erosion.

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.