Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 99% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
  - 90% Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
  - Xanthan gum
  - AC Blowing agent
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Zinc oxide desulfurizer
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst

###
Products

# 90% Zinc Oxide

- Previous

90% ceramic grade Zinc Oxide

Molecular Formula: ZnO

Molecular Weight: 81.38
CAS NO.: 1314-13-2
Properties: The product is white fine powder and can slowly absorb the water in the air.
Specification ( % )

Items | Index
standard | result
ZnO % | 90 | 90
water % | 1.2 | 1.0
Water soluble matter % | 0.5 | 0.7
Ignition Loss % | 1-4 | 1.0
HCl Insolubles % | 0.05 | 0.04
Pb %< = | 0.8 | 0.5
Mn %< = | 0.001 | 0.003
Cu %< = | 0.014 | 0.01
Residue on 45um Sieve %< = | 0.4 | 0.4
Cd%< = | 0.013 | 0.01
Fe%< = | 0.001 | 0.001

Use: For ceramic industry, enamel, rubber and other chemical industry application.
Storage: Store at a cool and dry place.
Packing: 25Kg woven bags lined with plastic bag( Or as clients' requirement ).

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.