### You are here:

COMPANY INTRODUCTION

Our value:

- Never compromise on design safety, integrity, efficiency, and reliability.
- Deliver compact and design and never sell customers more than they need.
- Give customers support whenever it is required.
- Never stop trying to improve our equipment, solutions and services.

Since 1990,From simple manual spraying to automatic powder spraying system.We can provide you with innovative, rational and economical solutions. We can support you with advanced technologies.Delivering the best powder coating equipments and turn-key solutions.
We’ve built thousands of optimal customized lines and systems for powder coating operations across China and around the world. Hanna’s list of satisfied clients includes successful small manufacturers, government organizations, and global corporations.
Our mainly products include: Manual powder coating machine, Automatic powder coating line, Spray painting equipment, Pretreatment System, Drying Oven, Powder Spraying Gun, Reciprocator, Fast Automatic Color Change Equipment, Powder Coating Booth, Powder Recovery Equipment, Conveyor Chains, Curing Oven, etc.All the systems are widely used on the applications of automotive, home and office appliance, machines industry, metal fabrications and so on.
1,Our staff includes coating system designers, powder and chemistry experts, control systems engineers, technical support personnel, installation technicians and experienced trainers.You won’t find a better combination of quality, value and support anywhere in this industry.
2,Each piece of equipment is built to meet your specific needs. To make sure you get the best results, our factory-authorized technician team will help you work through the details and get the results you need. We will design, build, deliver your automated system and if more services needed, we can help to install, fine-tune and train your operators to get premium results.
3,Our continuous research on the field as well as our constantly developing techniques and innovative nature of our engineering dpt. enable our customers to catch up to the latest developments by modernizing their equipment partly or wholly, so as to improve performance, increase profits and maintain their competitiveness in the world of trade.
WHY CHOOSE US
Our Advantages
*Pollution free operation.
*Safe to operate.
*Maximum recovery efficiency.
*Durability.
*Quick colour change.
1,Hanna intelligent gun, unique circuit board design, Complete solve the problem of workpiece powder grooves on the dead angle, groove with powder.
2,Hanna unique to the wind system which make the effective temperature difference control furnace temperature fluctuate 3 ℃, ensure that products without color difference,coating dose not fall off.
3,Hanna big cyclone recovery system powder recovery rate as high as99.2%,ensure no dust spillover.Unique fast color change powder supply center, change color only 10 to 15 minutes.
Our Services
* Professional Design
* Professional Scheme
* Professional Installation
* The warranty period of the equipment is three years, and any quality problems will occur during the quality guarantee period. Our company will replace the original equipment (parts) free of charge.The quality assurance period will provide the life service after the expiration.
* Within 24 hours after receiving service demand, by technical staff, has a rich experience by phone, email, video and other forms to provide project consulting, fault diagnosis and other instructional technology services, to achieve customer satisfaction.
Product After Sale Management System
* Training operation and maintenance personnel in organization
* Tracking understand and maintenance of mechanical equipment performance and use effect
* Assist customers to manage the production process and select the specification of process management
* Providing vulnerable parts at the factory price
* Lifetime after-sales service
* If equipment failure, in 24 hours (provincial) to solve the problem, and do a good record
* Three year warranty, lifelong repair.
A:
Heating source system, Combustion unit
Heating Sources: natural gas / liquefied gas / diesel / electricity / coal / biological particles and so on,optional.
Our burner is fast heating, high efficiency and be equipped with proportional adjustment, frequency conversion.
The reaction signal of the probe is automatically adjusted to the amount of fire, the temperature of the furnace is kept consistent and the temperature difference is controlled within ±3°.
The layout of the air supply &nbsp;reasonable, the furnace temperature should be uniform and the quality of the product is well stabilized.
B:
Pretreatment system
Types: Immersion / spraying optional
Customized design based on quality requirements: washing, chemical degreasing, chemical rust removal, phosphating, etching, shot blasting.
C:
Large cyclone fast automatic color change spray booth
Our color change powder supply center can achieves fast color change in 10 minutes, large cyclone powder recovery system, powder recovery rate is up to 99.2%, to ensure that there is no powder spillover outside the spray booth.
D:
Quick assembly filter recovery spray booth
Our filter recycling powder spray booth is designed with cylinders, convenient for
customers to quickly disassemble and change color, so that it improves work efficiency and will be your good choice.
E:
Curing oven system
Divided into bridge type curing oven and tunnel curing oven.
The tunnel curing oven effectively solves the problem of insufficient workshop height,
The tunnel furnace we produce has a wind curtain at both ends and the temperature of the furnace won’t dissipate to the out, which saves the fuel. This is our patent.
The curing oven we produce saves fuel and saves your production. Curing oven insulation boards are all plug-in boards, seamless docking, heat bridge transfer technology.
F:
Chain conveyor system:
The rail can be divided into 150 rails ≤ 30KG, 250 rails ≤ 50KG (single point lifting)
1，The drive unit in our high-end conveyor system uses a drive with a torque limiter. When the conveyor goes wrong, it can automatically stop. After the malfunction is removed, it can be restarted.
2，If the rail length is less than 180 meters, it will be driven by a single drive device. If the track is more than 180 meters, we recommend the double drive device. If the rail length exceeds 180 meters with a single drive device, then the track, chain, and tension parts will be problematic. We are at your point of view, providing you with the best design for saving time, labor, and long-term cost savings.
Copyright © 2020 Lanscend Technology Co., Ltd. All Rights Reserved.