### You are here:

# GCF Electric double Clipping Machine

- Previous
- Next

Description of GCF Electric double Clipping Machine

This Machine is made of high quality stainless steel,reasonable in structure, easy to clean.Special surface treatment, highlywear-proof.

Advanced controlling system:Equipped with man-machine interface,servomotor as drive,simple operation

Efficiency driving mode: The machine adopts successive driving mechanism, avoids that the parts worn too much .At the same time, the machine adopts intermittent driving mechanism

Convenient lubricating system

Low maintain cost

Advance：

1. The components in the area in contact with the product are food-safe

2. Advanced PLC Control , Easy operation and direct display;

3. Simple operation with SAFETY TOUCH and easy to clean

4. Adopted with Frequency Control: High speeds, Start stable, Low noise, Saving energy

5. Safety protect System，Burst detection with automatic machine stop

6. Widely used inmeat , food and non-food areas for the widest range of products.

Technical Parameters

Model | GCF
Speed (times/min) | 40-120
Voltage | 380V 50HZ
Power (kW) | 3
Air pressure | 0.5—0.6 MPa
Suit casing size | Flat Width:40-135mm Cal: 25mm-85mm
Suit clips： | the range of 15 and 18
The length of stretch | 36-100mm (optional)
The height of sealing | 980—1050 mm
External Dim. (mm) | 1200×900×1900mm
Weight (kg) | approx.560

## Product Inquiry of GCF Electric double Clipping Machine

- *Message

Related Products of GCF Electric double Clipping Machine

##### GCF Electric double Clipping Machine

##### TTT01

##### TTT02

##### 1234

##### IHAS

##### 123

Copyright © 2022 lanscend01 All Rights Reserved.