| Español |

Products List

- Anchorge System
  - Anchor Head
  - Anchor Plate
  - Oil Jack & Pump
  - Wedge (Grip)
- Hot-Dipped Galvanized Steel Strand
- Hot-Dipped Galvanized Steel Wire
- Prestressing Strand
  - Filled Epoxy-Coated Seven-Wire Prestressing Steel Strand
  - High-Tensile Prestressing Hot-dipped Galvanized Steel Strand
  - Low Relaxation Prestressed Concrete Steel Strand
  - Retarded Bonded Prestressing Steel Strand
  - Unbonded Prestressing Steel Strand
- Prestressed Concrete Steel Bar
- Prestressing Wire
  - High-Tensile Prestressing Hot-Dipped Galvanized Steel Wire
  - Prestressed Concrete Wire
- Zinc-5%Al Coated (Galfan) Steel Strand
- Zn-5% Al Coated Steel Wire

Home -> Anchorge System -> Oil Jack & PumpProducts

## Oil Jack & Pump

HEBEI LONGSHENG supply verious single-pull / multi-pull jack & matched pump,available ranging capacity from 27T to 650T with stroke length 200mm for 12.7/15.2/15.7 strand system.

- Oil Jack & Pump 01
- Oil Jack & Pump 02
- Oil Jack & Pump 03
- Oil Jack & Pump 04
- Oil Jack & Pump 05
- Oil Jack & Pump 06