| Welcome to HEBEI XIAOPENG !

| English |  | русский |  | Português |
E-maill: admin@hoistcn.com

Products List
Contact Us

| Taocheng Development Zone, Hengshui City, Hebei Province. China
| +86-318-5111881
| +86-318-5111551
| admin@hoistcn.com ktxfactory@163.com

Home -> MD1 Electric Wire Rope HoistProducts

# 20T MD electric wire rope hoist

<<Previous Next>>

China factory for CD/MD wire rope electric hoist, monorail crane hoist

We have been in this industry for over 20 years, with a lot of experience producing and exporting electric hoist.

Our factory mainly produce high quality electric hoist, with 1 year warranty. We are confident that you will satisfied with the quality and price. Our products have been sold to many countries, to several famous large companies.

CD, MD electric hoist can be widely used to hoist heavy projects, or installed on the straight or curve I steel beam of single girder crane. It made the electric hoist common in industrial and mine factory.

1. Features

1)Nanjing special motor and Nanjing motor factory.

2)Trolley wheel, 45 carbon steel, with frequency treatment, stronger and thicker.

3)Gear box cover adopts casing of automotive technology.

4)The surface have gone through special treatment, the surface is more bright and smooth.

5) For control box, the contactor is Schneider contactor.

6) With load limiter.

7) Inner drum,outside drum, gearbox cover is thicker.

Type | MD1 electric wire rope hoist
Capacity(t) | 0.5 | 1 | 2 | 3 | 5 | 10
Lifting Height(m) | 6-24 | 6-30 | 6-30 | 6-30 | 6-30 | 9-30
Lifting Speed(m/min) | 8/0.8 | 8/0.8 | 8/0.8 | 8/0.8 | 8/0.8 | 7/0.7
Running Speed(m/min) |  |  | 20,30 |  |  |
Wire rope Type | 6x37-4.8-180 | 6x37-7.4-180 | 6x37-11-155 | 6x37-13-170 | 6x37-15-200 | 6x37-15-200
Lifting Motor | Model | ZD1 12-4 ZDS1 0.2/1.5 | ZD1 22-4 ZDS1 0.2/1.5 | ZD1 31-4 ZDS1 0.4/3 | ZD1 32-4 ZDS1 0.4/4.5 | ZD1 41-4 ZDS1 0.8/7.5 | ZD1 51-4 ZDS1 1.5/13
Capacity(Kw) | 0.8 | 1.5 | 3 | 4.5 | 7.8 | 13.0
R.P.M(r/min) | 1380 | 1380 | 1380 | 1380 | 1400 | 1400
Running Motor | Model | ZDY1 11-4 | ZDY1 11-4 | ZDY1 12-4 | ZDY1 12-4 | ZDY1 21-4 | ZDY1 21-4
Capacity(Kw) | 0.2 | 0.2 | 0.4 | 0.4 | 0.8 | 0.8X2
R.P.M(r/min) | 1380 | 1380 | 1380 | 1380 | 1380 | 1380

2. Products show

* color can be different, yellow, blue

* drum can be round, square

* OEM service provide

* packing is plywood box

* Three times surface treatment, smooth and bright

* parts good quality

* pay attention to parts detail treatment

* good painting system

* well-organized production process

<<Previous Next>>
PRODUCT CATEGORY
GET IN TOUCH
HEBEI XIAOPENG HOISTING EQUIPMENT FACTORY
Address: Taocheng Development Zone, Hengshui City, Hebei Province. China.
Tel: +86-318-5111881
Fax: +86-318-5111551
Email: admin@hoistcn.com ktxfactory@163.com
Postcode: 053000
CONNECT WITH US

© 2016 HEBEI XIAOPENG HOISTING EQUIPMENT FACTORY | All Rights Reserved.