###
Products

# KUH-50

- Previous
- Next

Description

Manual Probes Features

● Perfect Accuracy: ±3% HV, ±1.5HR, ±3%HB

● Microscopic Indentation

● Support 360° quick measuring

● Result in 2 seconds

● Directly display measurement result, times count, maximum, minimal, average and deviation.

● Save 1000 groups measurement data, Save 20 groups calibration data for invoking, improve calibration efficiency

● Standards: DIN 50159; ASTMA1038 ; JB/T9377

Specifications:

Product Name | Ultrasonic Hardness Tester
Model | KUH50
Indenter | 136°Vickers Diamond Indenter
Loading Force | 2Kgf(Optional: 1Kgf, 5Kgf, 10Kgf)
Measuring Range | HB: 85-650;HV 80-1599; HRC 20-70;HRB: 41-100; HRA: 61-85.6 HS: 34.2-97.3;Mpa: 255-2180N/mm
Measuring Accuracy | HV:±3%HV; HRC:±1.5HRC; HB:±3%HB; HLD:±5HLD;
Measuring Direction | Support 360°
Data Storage | To save 1000-groups of measuring data and 20-groups of calibration data
Hardness Scale | HV、HB、HRC, HLD
Data Display | Loading force, Testing-times, Testing result, Average, Maximum、Minimum、Deviation and Conversion scale.
Hardness Indication | LCD display
Language Selection | English, German, French, Spanish, Japanese,Turkish etc.
Operating Environment | Temperature:-10℃~50℃; Humidity: 30%~80%R.H
Recharging Time Battery Usage | Approx. 8 hours Approx. 7 hours (no backlight)
Operating Voltage | DC 6V
Instrument Dimensions | 160x80x31mm
Net Weight | Approximate 500g（Without probe）

Manual Probe Specifications:

Probe Type | 1Kgf | 2Kgf | 5Kgf | 10Kgf
Remark | Optional | Standard | Optional | Optional
Loading force | 10N | 20N | 50N | 98N
Diameter | 22mm | 22mm | 22mm | 22mm
Length | 154mm | 154mm | 154mm | 154mm
Oscillating Rod Diameter | 2.4mm | 2.4mm | 3mm | 3mm
Roughness of measuring surface | Ra<3.2um | Ra<5um | Ra<10um | Ra<15um
Min weight of test material | 0.3kg | 0.3kg | 0.3kg | 0.3kg
Min thickness of test material | 2mm | 2mm | 2mm | 2mm

Related Products

##### KBT-10SA

##### KH-160

##### KH-500

##### KH-100S

##### KH-320

##### KH-260plus

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.