###
Products

# KH-100S

- Previous
- Next

Description

Features:

●Easy to operate, menu driven

●Large LCD display with backlight

●For most metals, and the metal’s name directly display on the screen.

●Based on the hardness HL value, conversion can be performed to HRB, HRC, HV, HB, HS and Tensile strength

●High accuracy ±0.5%

●Impact device D, DC, DL, C, D+15 and G are available for special applications

●Test at any angle, even upside down

●USB output and internal memory in a batch of 2000 average readings and optional Bluetooth printer

●Conforming to ASTM A 956

Measuring Range (table 1)

Materials | HL | HRC | HRB | HB | HS | HV
Steel & Cast Steel | 300-900 | 20.0-68.0 | 38.4-99.5 | 80-647 | 32.5-99.5 | 80-940
Alloy Tool Steel | 300-840 | 20.4-67.1 |  |  |  | 80-898
Stainless Steel | 300-800 | 19.2-62.4 | 46.5-101.7 | 85-655 |  | 85-802
Grey Cast Iron | 360-650 |  |  | 93-334 30D2 |  |
Spheroidal Iron | 400-660 |  |  | 131-387 30D2 |  |
Cast Aluminum | 174-560 |  |  | 20-159 10D2 |  |
Brass | 200-550 |  | 13.5-95.3 | 40-173 10D2 |  |
Bronze | 300-700 |  |  | 60-290 10D2 |  |
Copper | 200-690 |  |  | 45-315 10D2 |  |

Technical specifications:

Display functions | Hardness value, times, average indicator and average value, impact direction, type of impact device, memory, battery power consumption
Hardness parameter | HL, HRC, HRB, HV, HB, HS
Measuring range | See table 1
Optional Impact Device | DC/D+15/DL/C/G
Tensile Strength UTS range | δb from 370 to 2000 (106N/mm) (Steel only)
Materials | Steel & cast steel, Alloy tool steel, Stainless steel, Grey cast iron, Spheroidal iron ,Cast aluminum, Brass, Bronze, wrought copper alloy
Accuracy | +/-0.5% (HLD=800)
Memory | 2000 groups
Output | USB or Bluetooth printer
Display | 128╳64 LCD display with backlight
Impact Device Recognize | Auto
Power supply | 2 Pcs AAA alkaline battery
Working temp. | -20oC~+50 oC
Dimensions | 113 × 64 × 29 mm
Weight | 150g (include batteries)

# Standard delivery:

●Main unit

●Impact device D

●Test block with HLD value

●Software and cable

●Cleaning brush

●Small supporting ring

●Carrying case

●Operation manual

●Calibration certificate

Optional Accessories

Blue tooth Printer Impact devices

Related Products

##### KH-500

##### KUH-50

##### KBT-10SA

##### KH-320

##### KH-260plus

##### KH-220

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.