###
Products

# Electronic Stethoscope

Description

Introduction:

It is an easy to use electronic stethoscope designed to help locate the source of excess bearing and machine noise. It is a simple and at low cost solution which could save multiple hours of investigative and diagnostics work. It is an ideal listening device for finding the origin of mechanically generated noise in all types of applications. It has energy-saving, automatic shut-off function and an intelligent warning system to indicate low quantity of electricity. The whole body is designed in a soft curve form fit to human palm so as to be used comfortably.

★ Patent product - function of protecting hearing(limiting sound volume less than international environmental noise standard).

★ Effective energy-saving - 4 No.7 battery cells for 38 hours continuous work.

★ Intelligent low-quantity of electricity warning - when battery cells are about to be exhausted, the indicator fleshes so as to remind user to replace them.

★ Human naturalized design - the whole body is designed in a soft curve form fit to human palm so as to be used comfortably.

★ High-rank earphone-----of anti-noise

Application field:

●Capable of rapidly detecting mechanical noise from diesel engine, cylinder and vehicle ,accurately discover the failure position.

●Capable of detecting non-normal noise from driven engine, motor,etc.

●Capable of monitoring working states of auto pipeline in different enterprises, so as to insure the pipeline to work normally.

●Applicable in different chemical industries. Monitoring the flowing and jamming state in different pipelines.

●Capable of monitoring abnormal noise in boiler and reactor.

●Capable of distinguishing rapidly rotating state of different hearing.

●Applicable in shipping, shipbuilding industry and etc, monitoring working state of ships.

●Applicable in maintenance of vehicles in army.

●Capable of being a tool for domestic electric appliance.

Specification:

Frequency Range | 30Hz – 15KHz
Working Temp. | -10℃～+55℃
Output Volume | Digitally adjustable in 32 steps
Battery | 4 x AAA A cells
Battery life | Approx. 60 days
Dimensions | 220x 40 x 35mm
Probes | 1 x 284mm, 1 x 70mm

Related Products

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.