###
Products

# KGM1-F1

- Previous
- Next

Description

Hand held Gloss meters

Type: KGM1-F1 ( 60 °, 0.1 GU Resolution )
Description:
Small, stable, precise. AA-size battery.

Technical Parameters | Unit | Parameter
Reading Range | GU | 0.0～199.9
Deviation | GU | ±1.2
Measuring Area | mm2 | 20×10
Incidence Angle | Deg. | 60
Volume (L×W×H) | mm3 | 123×38×65
Main Weight | g | 300
Power supply | One AA-size battery, 1.2v-1.5v,Rechangeable or alkaline

Related Products

##### KGM1-C1

##### KGM1-S1

##### KGM1-F2

##### KGM3-F2

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.