###
Products

# ATB6

- Previous
- Next

Description

Hand held Thermal Imaging Camera

Features

- 2.4'' Digital Display Screen - Adjustable emissivity from 0.1 to1.0

- Units/date/time set - Selectable color palettes

- Visual/heat map image alignment - Image capture and image

- Led light allows the unit to be used in poor light - Auto power off

A djust the mixed image from 0% to 100%

Description

Model | ATB6
Display | 2.4 TFT LCD, 80 x 60 pixels
Infrared resolution | 60*60 (3600 pixels)
Detector resolution | 300,000 pixels
Field of view | 20°x 20°
Minimum focus length | 0.5m
Thermal sensitivity | 0.15ºC
Emissivity | Adjustable 0.1~1.0
Temperature measurement range | -20ºC ~300ºC / -4ºF~ 572ºF
Accuracy | ±2% or ±2.0ºC /3.6ºF of reading
Wavelength range | 8~14um
Image Frequency | 6HZ
Focus model | Fixed focus
Color palettes | Ironbow iridescence ,iridescence high contrast,Grayscale ,Grayscale inverted
Vision option | 25% step infrared to visional to infrared and visional image
Storage | SD card
Image file formats | Bmp
Operating Environment | -5 to 40°C (23 – 104°F), ≤ 80% Humidity
Emissivity | 0.1 – 1.0 adjustable
Batteries | Alkaline battery AA 1.5V*4
Battery life | 6 hours
Size /weight | 223 x 88 x 65 mm / 305 g

Related Products

##### ATH1

##### AT5X

##### AT3B

##### AT60S

##### AT15 & AT35

##### AT4 & AT8

- Previous
- Next

- Enquire Now

### Products List

Copyright ©KANG METER TECHNOLOGY CO,. LTD. All Rights Reserved.