###

- Next

# 3-Stages Hydrator

Description
KayeengXH hydrator/lime slaker is a core equipment to produce calcium hydroxide powder which absorbed domestic and foreign advanced technology, combined with the practice of design and manufacture. The structure of equipment is composed of a casing, a stirring shaft, transmission system, spraying system and control system.
And KayeengXH-C limeslaker is new style production equipment which performance reaches the advanced stage in the world. This type of limeslaker consists of three stages and dust collector to form one integral unit. The first stage is biaxial with shaft speed adjustable. The second and third stage are single shaft. It strengthens the mixture of material and water, enhance the ability of hydrating. The quicklime can be hydrated extremely and the quality of the products get maximize.
Technical Data
Capacity: 3～30tph
Residual Moisture: ＜1%
Fineness suitable for chemical
and building applications: according to the requirement, up to 95%≤90 micron
High BET: ≥40m2/gr.
Related Products

##### Hydration Equipment

Copyright © 2026 Hebei Leadership Friends Engineering and Technology Co., Ltd All Rights Reserved.