Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Filter Belt -> Polyester Linear Screen

## Polyester Linear Screen

- 22mesh
- 06702
- 07903
- 08602
- 09502

Polyester linear screen is mainly the 2-shed and 3-shed polyester plain woven fabric, which is widely used in special lines, such as paper pulps making, sulphate pulp packing and cardboard pulp, fiberboard plants as well as tailings disposal, colliery, food and medicine as filter belt.

Polyester Linear Screen
Weaving Type | Model | Thread Diameter (mm) | Density (No.s/cm) | Srength (N/cm) | Air Permeability (m ³/m ² h)
Warp | Weft | Warp | Weft
2-shed plain weaving fabric | 05082 | 0.75 | 0.8 | 4.7-5 | 4.8-5 | 940 | >20000
05102 | 1.0 | 1.0 | 4.7-5.2 | 4.3-5 | 1600 | >15000
06702 | 0.7 | 0.7 | 8 | 7 | ≧1600 | 11000
07102 | 0.7 | 1.0 | 6.6-7 | 4.3-4.6 | 1100 | >15000
08552 | 0.55 | 0.55 | 7.5-8 | 8.5-9 | 850 | 850-6500
09452 | 0.45 | 0.45 | 10 | 8.6 | 1600 | 16000
09502 | 0.5 | 0.5 | 8.5-9 | 10-10.5 | 750 | >10000
12502 | 0.5 | 0.5 | 13.5 | 8.5 | 1800 | 6500
3-shed plain weaving fabric | 08603 | 0.5 | 0.6 | 10 | 9 | 1600 | 14000
08903 | 0.9 | 0.9 | 7.8-8 | 5-5.5 | 2100 | 7500-8500
07803 | 0.7 | 0.8 | 8 | 8 | 1600 | 10000
20353 | 0.3 | 0.35 | 22 | 14.5 | 1200 | 13000
20403 | 0.3 | 0.4 | 22 | 14.5 | 1200 | 13500