Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Stainless Steel Filter Mesh -> Square Weave Mesh

## Square Weave Mesh

- DSC_0217
- DSC_0319
- DSC_1590
- 1
- DSC_1335
- DSC_1342

1. Stainless steel filter cloth

Features of stainless steel filter cloth:
Material: SS304, 304L, 316, 316L, etc
Square opening with standard sizes
Firm structure
Friction resistance
High strength
Corrosion resistance
Heat resistance
Applications of Stainless steel filter cloth:
Widely used for filtering of liquid, solid particles, powders, dust in grain, medicine, ceramic, glass, food, scientific research, mine, coal and other fields.
2. Stainless Steel Crimped Mesh
Features of stainless crimped mesh:
Material: low carbon steel wire, SS304. 304L, 316, 316L, brass wire, etc.
Crimped mesh is woven after crimping, so it firm and dutable with beautiful outlook.
Applications of Crimped Mesh:
Stainless steel crimped mesh is mainly used in screening in mine, coal industry, construction, oasting of flour food and meat, etc.

Crimped Mesh
Wire Gauge (BWG) | Aperture Size (mm) | Wire Dia. (mm) | Weight(Kg/m²)
8 | 30 | 4.06 | 6.00
8 | 25 | 4.06 | 7.00
8 | 20 | 4.06 | 8.00
8 | 15 | 4.06 | 1.00
8 | 12 | 4.06 | 13.000
8 | 10 | 4.06 | 15.000
10 | 30 | 3.25 | 4.00
10 | 25 | 3.25 | 4.70
10 | 20 | 3.25 | 5.80
10 | 15 | 3.25 | 7.40
10 | 10 | 3.25 | 10.000
12 | 30 | 2.64 | 2.70
12 | 12 | 2.64 | 3.20
12 | 20 | 2.64 | 3.90
12 | 15 | 2.64 | 5.00
12 | 10 | 2.64 | 7.00
14 | 20 | 2.03 | 2.38
14 | 15 | 2.03 | 3.10
14 | 12 | 2.03 | 3.70
14 | 10 | 2.03 | 4.35
14 | 8 | 2.03 | 5.22
14 | 6 | 2.03 | 6.52
14 | 4 | 2.03 | 8.68
14 | 3 | 2.03 | 10.400
16 | 15 | 1.63 | 2.03
16 | 10 | 1.63 | 2.90
16 | 8 | 1.63 | 3.50
16 | 6 | 1.63 | 4.40
16 | 4 | 1.63 | 5.99
18 | 12 | 1.22 | 1.43
18 | 10 | 1.22 | 1.68
18 | 8 | 1.22 | 2.05
18 | 6 | 1.22 | 2.62
18 | 4 | 1.22 | 3.62
18 | 3 | 1.22 | 4.48
20 | 12 | 0.91 | 0.82
20 | 10 | 0.91 | 0.96
20 | 8 | 0.91 | 1.18
20 | 5 | 0.91 | 1.78
20 | 4 | 0.91 | 2.15
20 | 3 | 0.91 | 2.69