Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Filter Belt -> Sludge Dewatering Belt

## Sludge Dewatering Belt

- 15905
- 16903
- 22903
- 26808

Sludge Dewatering Fabric is mainly used for sludge dewatering in sewage treatment factories. It has the characteristics of good water permeability, air permeability and non-revealed sludge, acid-resistance, alkali-resistance, heat resistance under 180 degrees. Due to its unique designing structure, the sludge can be get off easily after filtration, the fabric is cleaned easily and has a long service life.

Sludge Dewatering Fabric
Model | Thread Dia. (mm) | Density (No.s/cm) | Srength (N/cm) | Air Permeability (m ³/m ² h)
Warp | Weft | Warp | Weft
2470 | 0.5 | 0.7 | 24 | 9 | 2000 | 6130
27708 | 0.5 | 0.7 | 28 | 8.5 | 2100 | 4120
22903 | 0.5 | 0.9 | 23 | 5.5 | 2000 | 6800
16903 | 0.7 | 0.9 | 17 | 4.5 | 2200 | 7920
121103 | 0.9 | 1.1 | 12.5 | 3.8 | 3600 | 8610
26808 | 0.5 | 0.8 | 27 | 8.5 | 2100 | 5120
14803 | 0.7 | 0.8 | 14.2-15 | 4.2-5.5 | 2400 | 3900-8500
16803 | 0.7 | 0.8 | 15.6-16 | 4.5-6 | 2650 | 4500-6500
16904 | 0.7 | 0.9 | 15.6-16 | 4.2-5 | 2800 | 4000-8000
121054 | 0.7 | 1.05 | 12-12.4 | 4.2-4.8 | 3400 | 2000-4000
20703 | 0.5 | 0.7 | 20-20.6 | 6.5-8 | 1850 | 6000-10000
16704 | 0.7 | 0.7 | 16-16.4 | 8.5-9 | 2650 | 10000-12000
26908 | 0.5 | 0.9 | 26.4-27 | 6.5-7.5 | 2400 | 4500-6500