Polyester Filter Belt >>
Polyester Linear Screen
Spiral Dryer Fabric
Spiral Press Filter Belt
Sludge Dewatering Belt
Polyester Dryer Screen
Polyester Forming Fabric
Desulfurization Filter Cloth
Polyester Printing Mesh >>
Printing Mesh for Textile >>
Printing Mesh for T Shirts/Garme..
Printing Mesh for Flatbed Textil..
Printing Mesh for High-end Texti..
Printing Mesh for CDs/DVDs
Printing Mesh for Glass
Printing Mesh for Ceramics
Printing Mesh for Electronics >>
Printing Mesh for Printed Circui..
Prinitng Mesh for Membrane Switc..
Polyester/Nylon Filter Mesh
Stainless Steel Filter Mesh >>
Square Weave Mesh
Dutch Weave Mesh

Add: | Industrial Park Zone of South
| Anping County, Hebei Province,
| China.
Zip: | 053600
Tel: | +86-15369679157
Skype: | summerpfmscreen
E-mail: | info@pfmscreen.com
| sales@pfmscreen.com

Products
Home-> Polyester Filter Belt -> Spiral Dryer Fabric

## Spiral Dryer Fabric

According to the weaving, polyester dryer fabric can be divided into 3-shed, 4-shed; According to the category, polyester dryer fabric can be divided into one and a half layer, double-layer and flat wire fabric.
3-shed one and a half layer is suitable for drying papers less than 70g.
4-shed double-layer fabric is suitable for drying papers more than 70g.
Flat wire dryer fabric is suitable for the fore hearing box of the drying zone.

Polyester Dryer Fabric
Weaving Types | Model | Thread Dia. (mm) | Density (No.s/cm) | Srength (N/cm) | Air Permeability (m ³/m ² h)
Warp | Weft | Warp | Weft
3-shed | 22503 | 0.5 | 0.5 | 24 | 12 | 2000 | 8000
22453 | 0.45 | 0.45 | 24 | 13 | 2000 | 8500
24503 | 0.5 | 0.5 | 25 | 12 | 2000 | 7000
24453 | 0.45 | 0.45 | 25 | 13 | 2000 | 6700
4-shed | 20504 | 0.5 | 0.5 | 22 | 12 | 2000 | 15000
22504 | 0.5 | 0.5 | 24 | 12 | 2000 | 12000
24504 | 0.5 | 0.5 | 26 | 12 | 2100 | 11000
18504 | 0.5 | 0.5 | 20 | 11 | 1800 | 8000
round wire fabric | 4106 | 0.5 | 0.7 | 22.8 | 12.4 | 2200 | 6800
0.3
Flat wire fabric | 4106-1 | 0.58 | 0.35 | 21 | 15 | 2000 | 2500
0.37 | 0.68
4106-2 | 0.58 | 0.35 | 21 | 14 | 2000 | 3000
0.37 | 0.68
4106-3 | 0.58 | 0.35 | 21 | 13 | 2000 | 4000
0.37 | 0.68
4106-4 | 0.58 | 0.35 | 21 | 13.5 | 2000 | 3500
0.37 | 0.68