Water mist spray fog atomizing desinfecting channel for car truck vehicles

Trucks disinfection system 
1. Intelligent type, auto on/off. 
2. Double row design, efficiency.

Application Fields

Disinfection for the vehicles at the gate before they enter some certain places, such as pourltry farm,food processing factory and some special laboratory etc.

Features:

Fully automatic control,no need for super vision.

Unique design  driven by air,can still be used for winter time.

With dual-stage atomization principle, can  automatically empty the pipe and nozzle after using,no bloking.

Uniform droplet, well spread without dead-zone ,can completely cover and disinfect the vehicles.



Disinfection for Truck at The Gate
The disinfection channel The spray system with overarching sprayers tall enough for any kind of commercial truck to fit through with multiple sprayers on each line
Disinfection Gate for disinfecting vehicles, design for spraying any type of passing through vehicles like agricultural machinery, poultry trucks, passenger cars. It prevents the transfer of diseases to the farm, danger zone Unidoz Biosecurity Gate
Track disinfection curtain is the best bio-insurance available on the market. Compared to the disinfection mat, we have the ability to disinfect the passing vehicle, not just the lower part of the wheel. The vehicle is disinfected on all sides (360 ¡ã disinfection): the sides, the top, the front, the rear, the chassis.
In addition, it can be equipped with a 20m hose for spraying in inaccessible spots, and a system that allows disinfection channel to be used at low temperatures.
Made of powder-coated aluminum what makes it lightweight and easy to install. Reflective elements ensure adequate visibility after dark for passing drivers during night time
The Biosecurity Gate is designed for permanent or temporary installation at the entrance gate. Equipped with a 230V powered pump, which sucks in the predose disinfectant.
Equipment for Disinfection procedures for vehicles entering to pig farms, poultry farms, crop plants, industrial plants
Compared to manual disinfection Full disinfection of the vehicle takes seconds Recommended for protection against ASF African swine fever, H5N1 avian influenza, and many other diseases



MOBILE DISINFECTION GATE
Mobile Disinfection Gate DESTORmobil500. Decontamination by means of a mobile vehicle lock.
The mobile quick-fit gate impresses with highest quality. 

In order to prevent the spread of animal diseases, the fully automatic disinfection lock is set up on an outbreak farm by 2 persons within 20 minutes and works without manpower and with safe dosing.

Thus, the disinfection arch can be used as a rapid biosecurity measure on the farm in the event of an animal disease, or to prevent the spread of pathogens from flaying houses, wild game collection points or slaughterhouses.

The decontamination of vehicles and equipment has become an essential part of safety in recent years. In order to meet the requirements of fire brigades and technical relief organisations it is important to have appropriate equipment available. These primarily include components that can be used and operated in a short period of time by a small number of emergency personnel, regardless of the location. This is another field of application for the mobile decontamination lock, based on the G-decon concepts of fire brigades (Decon F).

Disinfection gate  Disinfection arch  Truck decontamination  Truck disinfection

Safe disinfection by means of fully-automatic operation.
The vehicle lock runs constantly with a reliable predetermined concentration of the disinfectant. The three-dimensional spraying nozzles are not susceptible to wind and guarantee a spread rate of 0.4 litres per square metre at a passage speed of 2.4 km/h. The offset arranged nozzles in the archway moisten the vehicle from above and from all sides. Full-surface wetting is guaranteed for all vehicle sizes and passenger cars, even with trailers. The powerful nozzles in the floor ramp ensure good underbody, tyre and wheel case cleaning. 

As soon as the vehicle approaches the disinfection arch, the high-efficiency sensors are activated and the nozzles immediately distribute the disinfectant at full pressure, even in front of the driver's cab and behind the rear.

Outbreak epidemic disease  Disinfection animal disease  Animal disease lock 
Quick assembly due to lightweight construction.
The transit gate is constructed as a modular lightweight system so that two persons can set up the complete disinfection lock in 20 minutes. All accessories are available and stored in sturdy transport boxes. The personnel do not need special training and can set up the gate on a mobile collection pan or an existing tray.

The spray arch consists of square tubes made of aluminium with an internal nozzle line. The pipes are first connected to each other on the floor and can be folded. They are attached to two brackets that are weighted down by filled barrels. The arch can be effortlessly pulled up by hand with a swivelling device.

The drive-over ramp consists of two floor traverses with an internal nozzle line and rubber feet that are placed beneath the disinfection arch. The sensors are then installed and all interconnections between components and storage container are established by simple couplings. The concentration of the disinfectant solution is set on the control unit and the drive-through lock works completely independently.

Vehicle Disinfection Channel:
--------------------------------

Performance in detail:
Square tube frames made of 100 mm aluminium have an internal nozzle string, light and stable, use of storm nozzles.
One aluminium hinged foot on each side serves to secure the arch and has a mounting bracket for a barrel to be filled for loading making the disinfection gate wind resistant.
The sensor system for the passage is attached to a quick-plug holder on the gate. It has an adjustment option and passage control for drive-through in one or both directions.
Constantly high pressure on the nozzles is generated by a multistage stainless steel centrifugal pump with 200 l/min.
The exact dosing of the disinfectant solution is carried out by a stepper motor pump with a setting range of 0.01 - 15 %, batches or time-dependent dosing can also be set. Water consumption is recorded on SD card.
The mixed solution is collected in a 1000 l intermediate buffer, the built-in floater triggers the automatic refill function.
Disinfection arch  Truck decontamination  Truck disinfection  Vehicle disinfection
Worldwide shipping
Our disinfection gates are used worldwide. In the Asian region, we ship by sea freight, e.g. to countries currently affected by the ASP epidemic, such as Cambodia or Thailand. There, the decontamination locks for trucks are mainly used in agricultural operations for pigs and poultry farms.

But the disinfection sheets are also used in Europe, e.g. in Greece, Poland or for the Luxembourg army to ward off epidemics.

The mobile version of the disinfection gate is already ideally prepared for export in a compact transport chassis.

The stationary truck locks can be safely shipped in a bundle of pipes and a Euro pallet.


Are the disinfection tunnels safe?

Now as various version of disinfection tunnels are springing up across the country, the biggest problems you will ask is that if the disinfectant it sprays safe? Or will the disinfectant burn you skin or harm to your body if inhaled?

Essentially these tunnels spray a mist of compound potassium peroxymonosulphate powder through right proportion,it¡¯s the same disinfectant as the bleach agent in the tap water you drink every day.

Currently ,there are many kinds of disinfectants in the market,you will find their application scope and functions as the following comparison:


===========================
vehicle disinfection mat
https://www.bg-safety.com/disinfection-products/vehicle-wheels-disinfection/

Technical Information
The Shoof Vehicle Disinfection Mat is supplied in two parts that are domed together along the centre line for use. There are stainless steel eyelets in the corners for securing to the roadway if required. The road surface must be smooth under the mat. Asphalt is excellent, chip seal is acceptable if it is fine chip. If the road is coarse chip seal, plain gravel or sand, it should be covered with plywood under the mat.

Directions for Use
To use for the first time, prepare about 40 litres of disinfectant solution in 20-litre jerry cans. Pour slowly on each side of the mat. (When the mat is new it can be slow to take in the solution.) For subsequent daily or twice-daily refilling, apply 20 litres to each side of the mat, or such amount as required.

Limited custom production available.

Dimensions & Capacity


---

Helps prevent the spread of infectious diseases such as Avian Influenza (Bird Flu), Equine Influenza, Foot & Mouth and Swine Flu. Also vital in reducing the transference of many other diseases such as salmonella, campylobacter and footpad dermatitis.

Disinfectant twin track HGV mats were used extensively in 2001 and 2007 against the foot and mouth outbreak. They have been specifically designed to disinfect the tyres of heavy goods vehicles and tractors. The traffic mats are extremely hardwearing are can withstand 50 or more heavy goods vehicles per day.

Note - For optimum performance it is imperative that the mats are fixed down securely to a firm, solid flooring using the fixings provided.

Specification
2 twin track mats per pack
Length - 3.5 metres
Manufactured from super absorbent matting
Hardwearing cover encased in PVC coated polyester envelope
Fixings provided
Effective & Economical
Evidence of reduced bacterial counts prove the effectiveness of dispensing disinfectants into treads of tyres
Replenish disinfectant as necessary
No wastage of disinfectant
Easy Installation
Laid on concrete or tarmac
Easy fix bolts provided
Dimensions & Sorbency
1m x 3.5m - 50 Litres sorbency
 
---
Available in three sizes: 60 x 90 cm, 180 x 90 cm and 230 x 47cm

COVID-19 Update: We are open, in stock and dispatching product daily. The best way to place your order is through our online shop.

Shop Now
The disinfectant mats are made up of two parts:

A 4cm thick, high density foam pad in a tough non-slip cover, designed to withstand heavy loads.
A unique waterproof sleeve to hold in the liquid. The sleeve is removable to allow thorough cleaning, which is not possible when the sleeve is sewn onto the pad.
Vehicle disinfectant matsThey are used in high health status buildings, dairies, fish farms, poultry sheds, food factories, horticulture units, vet practices, at agricultural events (including the Dairy Event) and farm open days.

Our disinfection mats:

Use 75% less solution than a conventional dip with no splashing and complete coverage
Are suitable for all disinfectant, foot care products and antibiotics
Are completely mobile and can be used on any flat surface
Are available to buy online three different sizes: 60 x 90cm, 180 x 90cm and 230 x 47cm
Our mats were used extensively during the foot and mouth crises in 2001 and 2007 by several big dairy companies, the National Trust, major race courses, DEFRA and even a film set!  More recently they have been providing protection against avian flu and strangles.


========================== 2c
medical office trash cans
https://www.bg-safety.com/others/pedal-trash-cans-and-trash-bags/medical-trash-can-1552.html

QuickMedical features heavy-duty trash cans for the medical exam or hospital room, and laboratory. With foot pedal and self-closing lids, the waste receptacles are convenient and clean. Available in baked epoxy, stainless steel, and red biohazard.



Infrared technology is already used widely in healthcare environments for activating
faucets and towel dispensers.  Now this proven technology enables you to freely open
and close the trash lid - without ever having to touch those nasty, contaminated lids!  
It's convenient.  It saves time.  And it enhances your infection control practices.  
Simply place your hand or trash within 10 inches of the infrared chip and
the lid opens instantly.  The lid closes tightly four seconds after use.

Touchless Trash Cans provide you with convenience and enhance your infection control
practices by eliminating the need to manually touch the lid each time you want
to discard trash.  Now you can reduce cross contamination and save time with
these "State of the Art" Touchless Trash Cans.  These sleek stainless steel and
plastic cans in various colors are ideal for both healthcare and commercial
applications where both convenience and function are important.

Other features include Manual Open/ Close buttons and power
saving On/ Off switch.  Garbage bag retainer ring tightly holds the
edge of the bag to prevent spillage.  Easily cleaned removable
plastic liners are included with all sizes.  

ABS Plastic Lid will not crack, change shape or change
color due to variations in climate.  The lid is designed to close
tightly, silently and efficiently.  Hidden compartment holds
batteries.  Add $2 for 4 optional D size Toshiba batteries.
Batteries last for about 10,000 uses or 1 year.*
(open & close)  Mfg. warranty on cans is 1 year.

---
Medical Waste Containers
A variety of options are available for meeting your medical waste disposal requirements, including large rollout Brute medical waste containers and smaller mobile step-on medical waste disposal containers. Whether you're looking for hospital waste containers or compact disposal containers for a physician's office, you'll find a wide range of sizes, shapes, and features from which to choose in our selection of medical waste disposal containers, waste bins, and trash receptacles.

View: Rubbermaid Defenders Step On Containers
Rubbermaid Defenders Step On Containers
A favorite of hospitals and doctors offices for many years the Defender line of hands free waste containers are made of high quality materials for many years of reliable service.

View: Brute Medical Waste Collection
Brute Medical Waste Collection
Collection of mobile and square Brute Medical waste collection containers. The square Brutes 3517 combo has passed DOT #178.603, #178.606 and #178.608 criteria for shipping of solid regulated medical waste.
---



===========================
battery powered backpack sprayer
https://www.bg-safety.com/disinfection-products/battery-powered-backpack-sprayer/


Battery-powered backpack sprayer. If you are trying to find the suited battery-powered backpack sprayer, the effort can be costly, tiring, costly, and a frustrating task. However, for you to discover what battery-powered backpack sprayer suits your needs, you require to understand what factors to consider as you purchase a battery-powered backpack sprayer today.

The threat to your plants is so real. They find it no more comfortable to live in a hostile and toxic environment as you do. If it is for commercial or for home use, you have to take care of the surroundings where you plant your plants.

Using a battery-powered backpack sprayer, you can dispense a dose of weed killing and pest destroying solutions rapidly and easily.

Table of Contents	
What to consider when selecting battery-powered backpack sprayer
1.Primary use
2. The manual or battery-powered backpack sprayer
3. Battery life
4. Type of pump
5. Safe and comfort
6. Spray wand
7. Ease of repair and has durability
What is the best battery powered backpack sprayer?
1. 105Ex Effortless Backpack Sprayer
2. Chapin 4-Gallon 24-volt Extended Spray Time Battery-powered Backpack Sprayer For Fertilizer, Herbicides, and Pesticides
3. Hudson 13854 Never Pump Back-Pack 4 Gallon Battery Operated Sprayer
4. Petra 4 Gallon Battery Powered Backpack Sprayer
5. M4 MY4SONS 4-Gallon Battery Powered Backpack Sprayer Wide Mouth
How to maintain your battery-powered backpack sprayer
Common parts of battery-powered backpack sprayer
How to charge the battery of the backpack sprayer
How to operate the battery backpack sprayer
How to spray using the backpack sprayer
How to store the battery-powered backpack sprayer properly
How to care for the battery
What to consider when selecting battery-powered backpack sprayer
1.Primary use
What is the primary use of your battery-powered backpack sprayer? If you are using mainly oil-based carriers or for woody plant control, you will need sprayer pumps, hoses, and oil-resistant seals. Battery-powered backpack sprayers must have durability, especially with multiple applicators using the same equipment.

2. The manual or battery-powered backpack sprayer
Manual sprayers are usually for treating new infestations. A battery-powered backpack sprayer will provide more convenience for large areas. The battery-powered backpack sprayer will ease off the pressure from manually pumping a handle to maintain pressure.

But, battery-powered backpack sprayers are commonly more expensive, heavier, and need more maintenance compared to manual sprayers.

If you decide to purchase a battery-powered backpack sprayer, make sure that the battery can handle both high and low sprayer psi output.

3. Battery life
The battery life of a battery-powered backpack sprayer will determine how long you can use the sprayer with just one single charge. Some products have a battery that can last up to ten hours with one single charge. Other products can last fewer than that.

4. Type of pump
Most backpack sprayers will come with a diaphragm pump or a piston pump. The piston pump is lower in price than diaphragm pumps. Piston pumps may not be suitable for herbicides.

If you are applying desiccant herbicide, the piston pump may wear out faster and need replacement. A diaphragm pump will provide ease of repair and durability with herbicides.

5. Safe and comfort
Features like a spray wand grip and a full-size pump handle help reduce user fatigue. A contoured tank and an adjustable, chemical resistant padded straps provide a comfortable fit for the user.

A padded harness has to be bought separately for some sprayers. Find Viton type rubber seals that resist softening and swelling that can cause leakage and pump breakdown.

6. Spray wand
A high-quality spray wand can withstand any factors that may cause leaks and can provide accurate application and comfort to the user. Find spray wands that accept the TeeJet caps and nozzles, that let the user choose from a numerous assortment of industrial-grade tips.

7. Ease of repair and has durability
The battery-powered backpack sprayer tank should be made of high-density polyethylene with UV protection for you to have a quality tank. Seals, other accessories, and hoses should be rated for additives and herbicides. Repair parts should be available online or at your local suppliers to replace components such as pumps.

What is the best battery powered backpack sprayer?
---
Enjoy 1.75 hours of continuous spraying with the Chapin 20-Volt Battery Backpack Sprayer. The 4 Gal. translucent poly tank comes with an extra-large 6 in. W mouth opening for easy filling and cleaning and a carrying handle built right into the cap. Cushion grip shut-off with built-in serviceable filter to assure that no debris can clog the nozzle. Deluxe padded shoulder straps. Offers 35 psi to 40 psi with a 35 ft. maximum horizontal spray stream. Additional batteries and chargers available through Black and Decker. Compatible with common fertilizers, weed killers and pesticides, you can trust Chapin to get the job done.

20-Volt BLACK+DECKER lithium-ion battery for 1.75-hours of continuous spraying
4 Gal. translucent poly tank with extra-large 6 in. W mouth opening for easy filling and cleaning
Cushion grip shut-off with 3 nozzles for a variety of applications
Built-in serviceable filter to prevent debris from clogging the nozzle
Deluxe padded shoulder straps
Compatible with common fertilizers, weed killers and pesticides
Powered by BLACK+DECKER
California residents see Prop 65 WARNINGS

---
Emission-free and whisper-quiet. Features powerful 12V pumps and a low dry weight, for tireless working. Equipped with a comfortable padded backpack support frame with wide shoulder straps. Ideal for conservatories and greenhouses.

Corrosion-Proof Plastic Tank
Ergonomic Handle
Manual Trigger
1 Year Guarantee
Vibration-Dampened Pressure Gauge
Impact-Resistant Enclosure
1.5m Long Hose


Landscape/Garden Maintenance Reviewer
Would you recommend this product? Yes
Overall Rating
4 out of 5
Value
3 out of 5
Features
4 out of 5
Performance
4 out of 5
Reliability
3 out of 5
Fed up Pumping
21 Jun 2018
By AHarroldDufftown
" Purchased this sprayer for my business, with a lot of spraying to do I like the idea of not having to constantly pump a handle. My first sprayer had a small hole in the lance which caused a small fine spray to come out, doing gardens with weedkiller this wasn't an option to like. However on contacting Screwfix to advise it was faulty I had to return the complete sprayer, I couldn't just get a replacement lance, nor swap it out with another in stock. Thoroughly tested my new sprayer and all appears to be good.
The plastic hose on the lance is not very flexible and you'll end up fighting it to get the correct direction to spray.
The biggest problem, and let down, is the battery. Every other professional battery operated device I've purchased has a removable battery and a slot in battery charger. This allows for easy charging, plus the option to have spare batteries. The Solo has a non removable battery, this means having to carry the whole sprayer near to a plug point to charge it, even the length of cable supplied on the charger is extremely short. Surely for this price you should have easily removable batteries.
Overall it has helped me greatly, but with a few annoying niggles. "