### You are here:

# work jacket

### Core Positioning

Engineered for high-risk environments including outdoor operations, warehousing & logistics, road construction, and emergency response. Combining fluorescent warning, intelligent reflection, and robust construction, this jacket creates "visible safety," ensuring personnel are seen and protected in complex surroundings.

- Next

Description

#### Design & Functional Highlights

1. Fabric System: Dual-Fabric Splicing for Optimal Performance

- Fabric 1 (Fluorescent Yellow Body): Crafted from high-density nylon, offering stain resistance and easy cleaning. Provides high-saturation fluorescent visibility for clear long-distance recognition during daylight hours.

- Fabric 2 (Black Splicing): Abrasion-resistant and tear-proof, reinforcing high-wear areas such as shoulders, cuffs, and hem to significantly extend product lifespan.

2. Reflection System: 360° Stereoscopic Warning

- Reflective Strips (Patch-Type): Silver-gray high-brightness reflective bands strategically layered across the chest, back, and both sleeves. Utilizing micro-prism technology for instant reflection, achieving a visibility range exceeding 500 meters in nighttime or low-light conditions.

- Reflective Edging (Hood Brim): Enhanced with reflective binding along the integrated hood edge and collar to improve head/neck contour recognition and eliminate "visual blind spots."

3. Structural Design: Human-Centered Details for All-Scenario Use

- Integrated Hood (Hook-and-Loop + Drawstring): Seamlessly attached to the jacket body. Features dual-adjustment (hook-and-loop + drawstring) at the opening for a secure fit across various head sizes—windproof and anti-drop. A rear drawstring (on the back panel) allows fine-tuning of the hood shape, compatible with safety helmets.

- Dual Pocket Configuration:

  - Chest Utility Pocket (Flap + Snap Button): Secure storage for essential tools (walkie-talkie, pens, cards).

  - Waist Side Pocket (with Zipper): Deep storage design prevents item loss, ideal for mobile phones, keys, and personal belongings.

- Cuff Adjustment (Fabric 2): Hook-and-loop or snap-button closure ensures a snug wrist fit—blocks cold wind ingress and prevents entanglement with external objects.

- Hem Adjustment (Fabric 1): Drawstring or snap-button tightening enhances thermal insulation and maintains a neat silhouette.

- Ergonomic Paneling: Three-dimensional splicing at high-mobility zones (shoulders, elbows) promotes joint flexibility and reduces restrictive drag during movement.

4. Critical Details: Subtle Yet Essential Safety Features

- Matching Stitching: All seams utilize thread matching the fluorescent yellow fabric, minimizing visual clutter while enhancing overall garment refinement.

- Waterproof Zipper + Matte Puller: Front closure features a black waterproof zipper with a matte black puller, providing water resistance and scratch protection.

- Industrial Context Photography: Presented against authentic warehouse and construction site backdrops to visually demonstrate "field-grade" protective performance.

#### Applicable Scenarios

- Industrial: Warehousing & Logistics, Ports & Terminals, Machinery Manufacturing, Electrical Maintenance.

- Transportation: Road Construction, Traffic Police Duty, Sanitation Operations, Railway Maintenance.

- Outdoor: Night Cycling, Mountaineering (where high-visibility is mandated

Related Products

##### High-Visibility Work Jacket

##### Work Safety Pants

##### Work Cotton Jacket

##### work jacket

##### Workwear Short Sleeve

##### Professional Workwear

##### Reflective jacket

##### Reflective T-shirt