### You are here:

# Silver reflective strip

100% synthetic fiber
Reflection coefficient: greater than 500CPL
Washing performance: Wash 35 times at 60 ℃ (ISO6330)
Wash 30 times at 75 ℃ (ISO6330) and 25 times at 90 ℃ (ISO15797)

Dry cleaning 30 times (ISO3175)

ENISO20471 ANSI107 OEKO-TEX100

- Previous
- Next

Description
Related Products

##### High brightness reflective strip

##### Grey reflective strip

##### Grey polyester cotton reflective strip

##### Grey synthetic fiber reflective strip

##### Reflective stripe

##### Silver reflective strip

##### High quality reflective strip