Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# cation polyacrylamide

- Next

Molecular Formula: (C3H5NO)n

Molecular Weight: 71.07

CAS No.: 9003-05-8

Apperance: White Power

Packaging Detail: PP bag with double layers of polyethlene film bag inside, 25kg per bag.

Delivery Detail: Within 15-20 days after receiving the payment.
Property And Application: Cationic polyacrylamide is mainly used as flocculants and dewatering reagents for industry waste water and sewage; retention aids and intensifier in paper making industry; waste water treatment in pharmaceutical, leather making, printing and dyeing industry waste water treatment, and organizer in textile industry.

Items | Anionic PAM | Cationic PAM | Non-Ionic PAM | Amphoteric PAM
Particle Size (MM) | 0.15 | 0.15 | 0.15 | 0.15
Dry Weight (%) | >89 | >89 | >89 | >89
Dissolution Time (Hour) | <1 | <1 | <1 | <1
Insoluble (%) | <0.2 | <0.2 | <0.2 | <0.2
Molecular Weight (Million) | 3-29 | 3-16 | 3-15 | 8-15
Relative Charge (%) | 10-40 | 5-80 | 3-10 | –
Anionic Charge (%) | – | – | – | 5-15
Cationic Charge (%) | – | – | – | 5-50
Residual AM (PPM) | <500 | <500 | <500 | <500
PH Value | 5-14 | 5-14 | 5-14 | 5-14

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.