Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - Oil Grade
  - Rubber Grade
- Zinc Oxide
  - Indirect Method Zinc Oxide
  - Direct Method Zinc Oxide
  - Particle Zinc Oxide
  - Nano Active Zinc Oxide
  - Feed Grade Zinc Oxide

###
Products

# Direct Method Zinc Oxide

- Previous
- Next

Direct Method Zinc Oxide

Molecular Formula: ZnO

Molecular Weight: 81.38
CAS NO.: 1314-13-2
Properties: The product is white fine powder and can slowly absorb the water in the air.
Specification ( % )

Items | Standards
1st Grade | 2nd Grade
ZnO % | 95-98 | 95-98
Moisture % | 0.7 | 0.7
Water Insolubles % | 0.5 | 0.7
Ignition Loss % | 1-4 | 1-4
HCl Insolubles % | 0.02 | 0.05
Pb %< = | 0.01 | 0.05
Mn %< = | 0.001 | 0.003
Cu %< = | 0.001 | 0.003
Residue on 45um Sieve %< = | 0.1 | 0.4
Specific Area /g = | 45 | 35
Bulk Density g/ml = | 0.35 | 0.4

Use: For rubber, paint, enamel, glass and other chemical industry application.
Storage: Store at a cool and dry place.
Packing: 25Kg woven bags lined with plastic bag( Or as clients' requirement ).

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.