Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 99% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
  - 90% Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
  - Xanthan gum
  - AC Blowing agent
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Zinc oxide desulfurizer
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase

###
Products

# Zinc oxide desulfurizer

- Previous
- Next

This product is mainly made of active zinc oxide, adding appropriate amount of auxiliaries and refining by special processing technology.

This product has the characteristics of wide use temperature, high purification degree, high sulfur capacity, high strength, high water vapor resistance and so on.

And this product is mainly used for gas, liquid hydrocarbon and synthetic gas and other raw materials purification and refining.

Under the conditions of industrial use, the hydrogen sulfide content of various raw material waste gas purified by this product can reach less than 0.1PPm, and the saturated sulfur capacity can reach 35%.

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.