Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - Oil Grade
  - Rubber Grade
- Zinc Oxide
  - Indirect Method Zinc Oxide
  - Direct Method Zinc Oxide
  - Nano Active Zinc Oxide
  - Feed Grade Zinc Oxide
- Potassium Carbonate
  - Potassium Carbonate
- Stearic Acid
  - Stearic Acid Single Pressed
  - Stearic Acid Double Pressed
  - Stearic Acid Triple Pressed
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- Soda Ash
  - Soda ash light
  - Soda Ash Dense
- Polyacrylamide
  - Anionic Polyacrylamide
  - cation polyacrylamide
  - Non-ionic Polyacrylamide
  - Amphoteric Polyacrylamide

###
Products

# Soda ash light

- Next

Molecular Formula: Na2CO3

Molecular Weight: 105.99

CAS No.: 497-19-8

Apperance: White powder or fine crystals.

Packaging Detail: PP bag with double layers of polyethlene film bag inside, 25kg per bag.

Delivery Detail: Within 15-20 days after receiving the payment.
Property: White powdered crystal, true specific gravity 2.533 (20°C),bulk density 0.90min.Easily soluble in water, maximum solubility at 35.4°C. The aqueous solution appears strong alkalinity. On exposure to air it easily absorbs moisture, carbon dioxide, and gradually forms sodium bicarbonate (caking soda).

Quality Standard: GB210.1-2004

Application:

Soda is an important chemical substance of white power or fine grains, which is easily soluble in water, it is used as a raw material in the production of bulding glass, soap, papers and as a cleaning agent; For blesching, and in the treatment of water.

Items | Spec
Total base content (as Na2CO3, on dry base) | ≥99.2%
Chlorides (as NaCL, on dry base) | ≤0.7%
Iron (as Fe, on dry base) | ≤0.035%
Insolubles in water | ≤0.03%
Loss on ignition | ≤0.8%
Fineness (180um) | ≥75%

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.