Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# Conversion catalyst

- Previous
- Next

This product is a bonded catalyst with nickel as active component and alumina as carrier.

This product is mainly suitable for the second stage conversion of gaseous hydrocarbon raw material with methane as the main body, the second stage conversion of light oil as the raw material and the pure oxygen conversion process of coke oven gas.

Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.