Welcome to Shijiazhuang Baisheng Chemical Co., Ltd

> ### Products List

- Basic Zinc Carbonate
  - 50% zinc carbonate
  - 54% zinc carbonate
  - 57% zinc carbonate
- Zinc Oxide
  - 99.7% Zinc Oxide
  - 95% Nano Zinc Oxide (20-100nm)
  - 95% active Zinc Oxide
  - 76% Feed Grade Zinc Oxide
- Zinc Oxide Desulfurization
  - zinc oxide desulphurizer
- Sewage treatment agent
  - Sodium Tripolyphosphate(STPP)
  - sodium gluconate
  - Gluconate
  - citric acid
  - PAC
  - PAM
  - AOS
  - Sodium Hexameta Phosphate(SHMP)
- Flue gas desulfurizer
  - Activated carbon desulfurizer
  - Nickel-molybdenum hydrogenation conversion catalyst
  - Room temperature dechlorination agent
  - Thermal protection catalyst
  - Conversion catalyst
  - Iron molybdenum hydrogenation catalyst
- Titanium Dioxide
  - Titanium Dioxide Rutile
  - Titanium Dioxide Anatase
- AC Blowing agent
  - AC Blowing agent
- Xanthan gum
  - Xanthan gum
- copper sulfate
  - copper sulfate

###
Products

# Activated carbon desulfurizer

- Next

This product is made of high quality activated carbon as the carrier, add a variety of additives, through special treatment, can work at room temperature, normal pressure or pressure.
This product has good removal effect on thiophene, carbon sulfide, mercaptan, thioether, disulfide and other organic sulfur and sulfur dioxide.
This product also has a strong removal effect on hydrogen sulfide, can also be regenerated several times under certain conditions, and efficient room temperature iron oxide desulfurizer used together, can achieve a true sense of room temperature fine desulfurization.
This product can be widely used for fine removal of organic sulfur in natural gas, gas, coke oven gas and other process gases.
Copyright © Shijiazhuang Baisheng Chemical Co., Ltd. All Rights Reserved.